uint8 LIGHT_CONST_OFF = 0
uint8 LIGHT_CONST_ON = 1
uint8 LIGHT_BREATH = 2
uint8 LIGHT_CUSTOM = 3

bool cmd_ctrl_allowed
uint8 front_mode
uint8 front_custom_value
uint8 rear_mode
uint8 rear_custom_value
